# Static Call Graph for image ..\Output\STM32F407_PROJ.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Sat May 16 10:25:37 2020

### Maximum Stack Usage = 64 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

CAN_Write ⇒ CAN_Transmit

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX0_IRQHandler from can_controller.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN_RX_IRQHandler_Callback from app_can.o(.text) referenced from app_can.o(.text)
  - CAN_Read from can_controller.o(.text) referenced from can_controller.o(.data)
  - CAN_Set_Controller from can_controller.o(.text) referenced from can_controller.o(.data)
  - CAN_Set_Interrupt from can_controller.o(.text) referenced from can_controller.o(.data)
  - CAN_Write from can_controller.o(.text) referenced from can_controller.o(.data)
  - CRYP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI15_10_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - Reset_Handler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f4xx.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(.text)

  SystemCoreClockUpdate (Thumb, 174 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> CAN_Set_Interrupt

  NVIC_Init (Thumb, 106 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> CAN_Set_Interrupt

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> main

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  CAN_DeInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> CAN_Set_Controller

  CAN_Init (Thumb, 276 bytes, Stack size 12 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CAN_Init
  [Called By]
  - >> CAN_Set_Controller

  CAN_FilterInit (Thumb, 258 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_FilterInit
  [Called By]
  - >> CAN_Set_Controller

  CAN_StructInit (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text))
  [Called By]

  - >> CAN_Set_Controller

  CAN_SlaveStartBank (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_DBGFreeze (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_TTComModeCmd (Thumb, 118 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Transmit (Thumb, 304 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_Transmit
  [Called By]
  - >> CAN_Write

  CAN_TransmitStatus (Thumb, 138 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_CancelTransmit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Receive (Thumb, 240 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_Receive
  [Called By]
  - >> CAN_Read

  CAN_FIFORelease (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_MessagePending (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_OperatingModeRequest (Thumb, 162 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Sleep (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_WakeUp (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetLastErrorCode (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetReceiveErrorCounter (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetLSBTransmitErrorCounter (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text))
  [Called By]

  - >> CAN_Set_Interrupt

  CAN_GetFlagStatus (Thumb, 120 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_ClearFlag (Thumb, 52 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetITStatus (Thumb, 310 bytes, Stack size 16 bytes, stm32f4xx_can.o(.text), UNUSED)
  [Calls]

  - >> CheckITStatus

  CAN_ClearITPendingBit (Thumb, 162 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text))
  [Called By]

  - >> CAN1_RX0_IRQHandler

  GPIO_DeInit (Thumb, 220 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> CAN_Set_Controller

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> CAN_Set_Controller

  RCC_DeInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 222 bytes, Stack size 20 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> CAN_Set_Controller

  RCC_AHB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> CAN_Set_Controller

  RCC_APB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 72 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> CAN_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  main (Thumb, 44 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = main ⇒ app_can_tx_test
  [Calls]
  - >> NVIC_SetVectorTable
  - >> app_can_tx_test
  - >> app_can_rx_test
  - >> app_can_init
  - >> Systick_OsPeriod_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  Systick_DrvInit (Thumb, 42 bytes, Stack size 0 bytes, systick.o(.text), UNUSED)

  Systick_OsPeriod_Init (Thumb, 94 bytes, Stack size 20 bytes, systick.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Systick_OsPeriod_Init
  [Called By]
  - >> main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SysTick_Handler (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  register_can_controller (Thumb, 34 bytes, Stack size 0 bytes, app_can.o(.text))
  [Called By]

  - >> CAN1_contoller_add

  CAN_RX_IRQHandler_Callback (Thumb, 54 bytes, Stack size 24 bytes, app_can.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN_RX_IRQHandler_Callback
  [Calls]
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - app_can.o(.text)

  app_can_init (Thumb, 28 bytes, Stack size 8 bytes, app_can.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = app_can_init ⇒ CAN1_contoller_add
  [Calls]
  - >> CAN1_contoller_add
  [Called By]
  - >> main

  app_can_tx_test (Thumb, 122 bytes, Stack size 40 bytes, app_can.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_can_tx_test
  [Called By]
  - >> main

  app_can_rx_test (Thumb, 114 bytes, Stack size 40 bytes, app_can.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = app_can_rx_test
  [Called By]
  - >> main

  CAN_Baud_Process (Thumb, 84 bytes, Stack size 8 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_Baud_Process
  [Called By]
  - >> CAN_Set_Controller

  CAN_Set_Controller (Thumb, 222 bytes, Stack size 40 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = CAN_Set_Controller ⇒ GPIO_PinAFConfig
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> CAN_StructInit
  - >> CAN_FilterInit
  - >> CAN_Init
  - >> CAN_DeInit
  - >> CAN_Baud_Process
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Address Reference Count : 1]
  - can_controller.o(.data)

  CAN_Set_Interrupt (Thumb, 70 bytes, Stack size 16 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CAN_Set_Interrupt ⇒ NVIC_Init
  [Calls]
  - >> CAN_ITConfig
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  [Address Reference Count : 1]
  - can_controller.o(.data)

  CAN_Read (Thumb, 28 bytes, Stack size 16 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN_Read ⇒ CAN_Receive
  [Calls]
  - >> CAN_Receive
  [Address Reference Count : 1]
  - can_controller.o(.data)

  CAN_Write (Thumb, 88 bytes, Stack size 56 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = CAN_Write ⇒ CAN_Transmit
  [Calls]
  - >> CAN_Transmit
  [Address Reference Count : 1]
  - can_controller.o(.data)

  CAN1_RX0_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN1_RX0_IRQHandler
  [Calls]
  - >> CAN_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_contoller_add (Thumb, 10 bytes, Stack size 8 bytes, can_controller.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN1_contoller_add
  [Calls]
  - >> register_can_controller
  [Called By]
  - >> app_can_init

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> CAN_RX_IRQHandler_Callback

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> CAN_RX_IRQHandler_Callback

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 220 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  CheckITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)
  [Called By]

  - >> CAN_GetITStatus

  ### Undefined Global Symbols