1. 框架
1.1 硬件协议简介
1.2 驱动框架
1.3 bus-drv-dev模型及写程序
a. 设备的4种构建方法
a.1 定义一个i2c_board_info, 里面有:名字, 设备地址
    然后i2c_register_board_info(busnum, ...)   (把它们放入__i2c_board_list链表)
    			list_add_tail(&devinfo->list, &__i2c_board_list);

	链表何时使用：
	i2c_register_adapter > i2c_scan_static_board_info > i2c_new_device    				

    使用限制：必须在 i2c_register_adapter 之前 i2c_register_board_info
	所以：不适合我们动态加载insmod

a.2 直接i2c_new_device, i2c_new_probed_device
a.2.1 i2c_new_device        : 认为设备肯定存在
a.2.2 i2c_new_probed_device ：对于"已经识别出来的设备"(probed_device)，才会创建("new")
i2c_new_probed_device
	probe(adap, addr_list[i])   /* 确定设备是否真实存在 */
	info->addr = addr_list[i];
	i2c_new_device(adap, info);

a.3 从用户空间创建设备
创建设备
echo at24c08 0x50 > /sys/class/i2c-adapter/i2c-0/new_device

导致i2c_new_device被调用

删除设备
echo 0x50 > /sys/class/i2c-adapter/i2c-0/delete_device

导致i2c_unregister_device

a.4 前面的3种方法都要事先确定适配器(I2C总线,I2C控制器)
    如果我事先并不知道这个I2C设备在哪个适配器上，怎么办？去class表示的所有的适配器上查找
    有上一些I2C设备的地址是一样，怎么继续分配它是哪一款？用detect函数

static struct i2c_driver at24cxx_driver = {
	.class  = I2C_CLASS_HWMON, /* 表示去哪些适配器上找设备 */
	.driver	= {
		.name	= "100ask",
		.owner	= THIS_MODULE,
	},
	.probe		= at24cxx_probe,
	.remove		= __devexit_p(at24cxx_remove),
	.id_table	= at24cxx_id_table,
	.detect     = at24cxx_detect,  /* 用这个函数来检测设备确实存在 */
	.address_list	= addr_list,   /* 这些设备的地址 */
};

    
去"class表示的这一类"I2C适配器，用"detect函数"来确定能否找到"address_list里的设备",
如果能找到就调用i2c_new_device来注册i2c_client, 这会和i2c_driver的id_table比较，
如果匹配，调用probe

i2c_add_driver
	i2c_register_driver
		a. at24cxx_driver放入i2c_bus_type的drv链表
		   并且从dev链表里取出能匹配的i2c_client并调用probe
		driver_register
			
		
		b. 对于每一个适配器，调用__process_new_driver
		   对于每一个适配器，调用它的函数确定address_list里的设备是否存在
		   如果存在，再调用detect进一步确定、设置，然后i2c_new_device
		/* Walk the adapters that are already present */
		i2c_for_each_dev(driver, __process_new_driver);
			__process_new_driver
				i2c_do_add_adapter
					/* Detect supported devices on that bus, and instantiate them */
					i2c_detect(adap, driver);
						for (i = 0; address_list[i] != I2C_CLIENT_END; i += 1) {
							err = i2c_detect_address(temp_client, driver);
										/* 判断这个设备是否存在：简单的发出S信号确定有ACK */
										if (!i2c_default_probe(adapter, addr))
											return 0;
										
										memset(&info, 0, sizeof(struct i2c_board_info));
										info.addr = addr;	
										
										// 设置info.type
										err = driver->detect(temp_client, &info);
					
										i2c_new_device


b. 驱动的写法

2. 完善设备驱动程序

3. 不自己写驱动直接访问

Device Drivers
	 I2C support
		<*>   I2C device interface

4. 编写"总线(适配器adapter)"驱动

Device Drivers
	 I2C support
	 	I2C Hardware Bus support
	 		< > S3C2410 I2C Driver

nfs 30000000 192.168.1.123:/work/nfs_root/uImage_noi2cbus; bootm 30000000
