; Installation inf for the SEC SOC S3C2443X USB 2.0 Bulk IO Test B/D

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%ProviderName%
DriverVer=03/21/2007

[SourceDisksNames]
1="USB Downloader Installation Disk for SEC SOC",,,

[SourceDisksFiles]
SECUSB2.sys = 1
SECUSB2.inf = 1

[Manufacturer]
%MfgName%=SystemLsi

[SystemLsi]
%USB\VID_04E8&PID_1234.DeviceDesc%=SECUSB2.Dev, USB\VID_04E8&PID_1234
%USB\VID_04E8&PID_6400.DeviceDesc%=SECUSB2.Dev, USB\VID_04E8&PID_6400

;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
SECUSB2.Files.Ext = 10,System32\Drivers
SECUSB2.Files.Inf = 10,INF

[SECUSB2.Dev]
CopyFiles=SECUSB2.Files.Ext, SECUSB2.Files.Inf
AddReg=SECUSB2.AddReg

[SECUSB2.Dev.NT]
CopyFiles=SECUSB2.Files.Ext, SECUSB2.Files.Inf
AddReg=SECUSB2.AddReg

[SECUSB2.Dev.NT.Services]
Addservice = SECUSB2, 0x00000002, SECUSB2.AddService

[SECUSB2.AddService]
DisplayName    = %SECUSB2.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\SECUSB2.sys
LoadOrderGroup = Base

[SECUSB2.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SECUSB2.sys
HKLM,"System\Currentcontrolset\Services\SECUSB2\Parameters","MaximumTransferSize",0x10001,4096
HKLM,"System\Currentcontrolset\Services\SECUSB2\Parameters","DebugLevel",0x10001,2


[SECUSB2.Files.Ext]
SECUSB2.sys

[SECUSB2.Files.Inf]
SECUSB2.Inf


;---------------------------------------------------------------;

[Strings]
ProviderName="SEC AP application Team"
MfgName="SEC, SYSTEM LSI"
USB\VID_04E8&PID_1234.DeviceDesc="x210"
USB\VID_04E8&PID_6400.DeviceDesc="x210"
SECUSB2.SvcDesc="SECUSB2.sys, SEC SOC USBD Driver"

