[Version]                  ; Required section
Signature = "$Windows NT$"
Provider = "Marvell"
CESignature = "$Windows CE$"

[CEDevice.pocket.arm]
ProcessorType  = 2577
UnsupportedPlatforms = "HPC","Jupiter"
VersionMin = 4.00 ; version 4.0
VersionMax = 4.99

[DefaultInstall]           ; Required section
AddReg = RegSettings.All
CopyFiles = Files.ARM

[Files.ARM]
SDIO8686.dll,,,0


[SourceDisksNames]                   ; Required section
1 = ,"Common files",,.


[SourceDisksFiles]         ; Required section
SDIO8686.dll=1


[DestinationDirs]             ; Required section
;Shortcuts.All = 0,%CE2%\Help  ; set to \Windows\Help
Files.ARM = 0,%CE2%        ; \Windows

[CEStrings]                ; Required section
AppName = "SDIO8686 Driver"
InstallDir = %CE2%

[RegSettings.All]
HKLM,Drivers\SDCARD\ClientDrivers\Custom\MANF-02DF-CARDID-9103-FUNC-1,Dll,0x00000000,"SDIO8686.dll"
HKLM,Drivers\SDCARD\ClientDrivers\Custom\MANF-02DF-CARDID-9103-FUNC-1,Prefix,0x00000000,"NDL"
HKLM,Drivers\SDCARD\ClientDrivers\Custom\MANF-02DF-CARDID-9103-FUNC-1,Instance0,0x00000000,"SDIO8686:SDIO86861"

HKLM,Comm\SDIO8686,DisplayName,0x00000000,"Marvell SDIO8686 Wireless Card"
HKLM,Comm\SDIO8686,Group,0x00000000,"NDIS"
HKLM,Comm\SDIO8686,ImagePath,0x00000000,"SDIO8686.dll"

HKLM,Comm\SDIO8686\Linkage,Route,0x00010000,"SDIO86861"

HKLM,Comm\SDIO86861,DisplayName,0x00000000,"Marvell SDIO8686 Wireless Card"
HKLM,Comm\SDIO86861,Group,0x00000000,"NDIS"
HKLM,Comm\SDIO86861,ImagePath,0x00000000,"SDIO86861.dll"

HKLM,Comm\SDIO86861\Parms,BusNumber,0x00010001,0
HKLM,Comm\SDIO86861\Parms,BusType,0x00010001,0	; WinCE4.x only
HKLM,Comm\Tcpip\Linkage,Bind,0x00010000,"ppp","SDIO86861"

; setup card parameters
HKLM,Comm\SDIO86861\Parms,NetworkAddress,0x00000000,""
HKLM,Comm\SDIO86861\Parms,"PowerMode",0x00010001,0 ; 0 = off, 1 = on
HKLM,Comm\SDIO86861\Parms,"ExtendedScan",0x00010001,1 ; 0 = off, 1 = on
HKLM,Comm\SDIO86861\Parms,"FragThsd",0x00010001,0x92A
HKLM,Comm\SDIO86861\Parms,"RTSThsd",0x00010001,0x92A

; following is for BT co-existence testing
HKLM,Comm\SDIO86861\Parms,"BTMode",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTAntennaConfig",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTFrequencyConfig",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTWLANTxPriorityLo",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTWLANTxPriorityHi",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTWLANRxPriorityLo",0x00010001,0
HKLM,Comm\SDIO86861\Parms,"BTWLANRxPriorityHi",0x00010001,0

; adhoc starter default channel
HKLM,Comm\SDIO86861\Parms,"AdhocDefaultChannel",0x00010001,6
; adhoc starter WiFi test datarate modify or not 
HKLM,Comm\SDIO86861\Parms,"AdhocWiFiDataRate",0x00010001,0

;SetSD4BIT: Please set 1, SetSD1BIT: Please set 0, default SetSD1BIT
HKLM,Comm\SDIO86861\Parms,"SetSD4BIT",0x00010001,0

;Set the value of SdioIstThread
HKLM,Comm\SDIO86861\Parms,"SdioIstThread",0x00010001,0x65

;Set the value of AvoidScanTime after connected
HKLM,Comm\SDIO86861\Parms,"AvoidScanTime",0x00010001,10000

;Set ACTIVE_ROAMING
HKLM,Comm\SDIO86861\Parms,"bActiveRoamingScanOneChannel",0x00010001,1
HKLM,Comm\SDIO86861\Parms,"bLinkLostScanOneChannel",0x00010001,1

;Set NEW_RSSI parameters
HKLM,Comm\SDIO86861\Parms,"ulRSSIThresholdTimer",0x00010001,5000
HKLM,Comm\SDIO86861\Parms,"RSSI_Range",0x00010001,10

;Set ACTIVE_ROAMING with BackGround Scan
HKLM,Comm\SDIO86861\Parms,"bActiveRoamingwithBGSCAN",0x00010001,0

;Set the value of Enable80211D
HKLM,Comm\SDIO86861\Parms,"Enable80211D",0x00010001,0

;Set the value of LocalListenInterval
HKLM,Comm\SDIO86861\Parms,"LocalListenInterval",0x00010001,0

; default TCP/IP parameters
HKLM,Comm\SDIO86861\Parms\TcpIp,"EnableDHCP",0x00010001,1
HKLM,Comm\SDIO86861\Parms\TcpIp,"DefaultGateway",0x00010000,""
HKLM,Comm\SDIO86861\Parms\TcpIp,"UseZeroBroadcast",0x00010001,0
HKLM,Comm\SDIO86861\Parms\TcpIp,"IpAddress",0x00010000,"0.0.0.0"
HKLM,Comm\SDIO86861\Parms\TcpIp,"Subnetmask",0x00010000,"255.255.255.0"





