;CODEPAGE=1252

[EN]
INTF0262=AVRCP Control
AVRP0100=Make TCPMP supports AVRCP
AVRP0101=AVRCP Enabled
AVRP0102=Play
AVRP0103=Pause 
AVRP0104=Prev
AVRP0105=Next
AVRP0106=Backward
AVRP0107=Forward
AVRP0108=Off Screen when Headset Button pressed
AVRP0109=Auto toggle A2DP Mode
AVRP0110=You have set "Auto toggle A2DP Mode",when you connect a Headset and run TCPMP,it will toggle A2DP output automaticlly.\n\nNOTICE:If TCPMP is already opened while Headset connecting,you must restart TCPMP to take effect.
AVRP0111=Lock keypad while Screen Off
AVRP0112=Stop
