; ==============================================================================
;   Ralink Technology Inc.
;   5F, No. 36 Tai-yuan Street
;   Jhu-bei City, Hsin-chu County 302,
;   Taiwan, R.O.C.
;
;   (c) Copyright 2002-2008, Ralink Technology, Corp.
;
;   All rights reserved. Ralink's source code is an unpublished work and the
;   use of a copyright notice does not imply otherwise. This source code
;   contains confidential trade secret material of Ralink Tech. Any attemp
;   or participation in deciphering, decoding, reverse engineering or in any
;   way altering the source code is stricitly prohibited, unless the prior
;   written consent of Ralink Technology, Corp. is obtained.
; ==============================================================================
;   File:   RT2870.reg
;   Author: Claude Lee
; ==============================================================================
[HKEY_LOCAL_MACHINE\Comm\RT2870]
    "DisplayName"="RT2870 b/g/n Wireless LAN Driver"
    "Group"="NDIS"
    "ImagePath"="RT2870.dll"

[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\Default\Default\Default\RT2870]
    "Dll"="RT2870.DLL"

[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\RT2870]
    "Dll"="RT2870.DLL"
;
; Add "Flags" if hive-based registry is enabled
;
    ;"Flags"=dword:1000

[HKEY_LOCAL_MACHINE\Comm\RT28701\Parms]
;
;
; "CustomizedControlFlag"=0: Use internal table, 1: Use external pair, 2: both
;
    ;   "CustomizedVID"=dword:148f          ; hex
    ;   "CustomizedPID"=dword:2673          ; hex
    ;   "CustomizedControlFlag"=dword:0     ; 0: Use internal table, 1: Use external pair, 2: both

    "BusNumber"=dword:0
    "BusType"=dword:0
;
    "OpMode"=dword:0
    "WirelessMode"=dword:5
    "Channel"=dword:1
    "CountryRegion"=dword:5
    "CountryRegionABand"=dword:7
    "RtsThresh"=dword:92B
    "FragThresh"=dword:92A
    "Encryption"=dword:0
    "AuthenType"=dword:0
    ;"ShowHiddenSSID"=dword:0
    "AutoReconnect"=dword:1
    "NetworkType"=dword:1
    "SSID"="RT2870AP"
    ;"PreambleType"=dword:0
    ;"ShortSlot"=dword:1
    ;"BGProtection"=dword:0
    ;"TurboRate"=dword:0
    ;"AdhocOfdm"=dword:0
; 11n
    ;"RDG"=dword:1
    ;"AllowBW40InBGBand"=dword:1    
    "BACapability"=dword:07034020
    "TransmitSetting"=dword:2ba15

    "ProviderName"="Ralink Technology, Inc."
    "VendorDesc"="RT2870 802.11 b/g Wireless Card."
	"UseRaSupplicant"=dword:0
    "WEPKeyUse"=dword:1
    "WEPKey1"=""
    "WEPKey2"=""
    "WEPKey3"=""
    "WEPKey4"=""

[HKEY_LOCAL_MACHINE\Comm\RT28701\Parms\TcpIp]
    "EnableDHCP"=dword:0
    ;"DefaultGateway"=multi_sz:"192.168.1.1"
    ;"IpAddress"=multi_sz:"192.168.1.210"
    ;"Subnetmask"=multi_sz:"255.255.255.0"
    ;"DNS"="192.168.1.1"
    ;"WINS"=""

;
; Strong recommend install 2007M6 QFE, if you want to higer USB performance
;
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\PCI\Template\EHCI]
    ;"IntThreshCtrl"=dword:1        ; 1~8 microframe   ( 1 microframe = 125us)
