[HKEY_LOCAL_MACHINE\Drivers\PCMCIA\EAGLEND5]
   "Dll"="ndis.dll"
   "Prefix"="NDS"
   "Miniport"="EAGLEND5"

[HKEY_LOCAL_MACHINE\Drivers\PCMCIA\Detect\101]
   "Dll"="eaglend5.dll"
   "Entry"="DetectMrvDrv"

[HKEY_LOCAL_MACHINE\Comm\EAGLEND5]
   "DisplayName"="EAGLEND5"
   "Group"="NDIS"
   "ImagePath"="EAGLEND5.dll"

;
; Template for the PCI bus driver
;

[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\PCI\Template\EAGLEND5]
   "Dll"="NDIS.dll"
   "Entry"="NdisPCIBusDeviceInit"
   "IsrDll"="giisr.dll"
   "IsrHandler"="ISRHandler"
   "Class"=dword:02
   "SubClass"=dword:80
   "ProgIF"=dword:0
   "PortIsIO"=dword:0
   "PortOffset"=dword:00000C88
   "PortSize"=dword:4
   "PortMask"=dword:ffffffff
   "VendorID"=multi_sz:"1638"
   "DeviceID"=multi_sz:"1100"

[HKEY_LOCAL_MACHINE\Comm\EAGLEND5\Linkage]
   "Route"=multi_sz:"EAGLEND51"

[HKEY_LOCAL_MACHINE\Comm\EAGLEND51\Parms]
   "PowerMode"=dword:0
   "FragThsd"=dword:3E8
   "RTSThsd"=dword:1F4
   "NetworkAddress"=""

; default TCP/IP settings
[HKEY_LOCAL_MACHINE\Comm\EAGLEND51\Parms\TcpIp]
   "EnableDHCP"=dword:1
   ; This should be MULTI_SZ
   "DefaultGateway"=""
   ; Use zero for broadcast address? (or 255.255.255.255)
   "UseZeroBroadcast"=dword:0
   ; Thus should be MULTI_SZ, the IP address list
   "IpAddress"="192.168.0.99"
   ; This should be MULTI_SZ, the subnet masks for the above IP addresses
   "Subnetmask"="255.255.255.0"