; Copyright (c) 2005 Marvell Corporation.  All rights reserved.
;
;
; THIS CODE AND INFORMATION IS PROVIDED "AS IS" WITH
; WARRANTY OF ANY KIND, EITHER EXPRESSED OR IMPLIED, 
; INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF 
; MERCHANTABILITY AND/OR FITNESS FOR A PARTICULAR PURPOSE.
;


; registry keys for the NDIS driver
[HKEY_LOCAL_MACHINE\Comm\GSPI8385]
   "DisplayName"="Marvell 802.11 GSPI Adapter"
   "Group"="NDIS"
   "ImagePath"="GSPI8385.dll"

[HKEY_LOCAL_MACHINE\Comm\GSPI8385\Linkage]
   "Route"=multi_sz:"GSPI83851"

    ; instance 1 information
[HKEY_LOCAL_MACHINE\Comm\GSPI83851]
   "DisplayName"="Marvell 802.11 GSPI Adapter"
   "Group"="NDIS"
   "ImagePath"="GSPI8385.dll"
	
    ; instance 1 parameters
[HKEY_LOCAL_MACHINE\Comm\GSPI83851\Parms]
   "BusNumber"=dword:0
   "BusType"=dword:0
IF _WINCEOSVER=400
      ; .NET needs this bus type
   "BusType"=dword:0
ENDIF

IF _WINCEOSVER=410
       ; .NET needs this bus type
   "BusType"=dword:0
ENDIF

IF _WINCEOSVER=420
       ; .NET needs this bus type
   "BusType"=dword:0
ENDIF


IF _WINCEOSVER=300
       ; CE 3.0 or PocketPC needs this bus type
   "BusType"=dword:8
ENDIF


    ; TCPIP linkage to instance 1 adapter
[HKEY_LOCAL_MACHINE\Comm\Tcpip\Linkage]
    "Bind"=multi_sz:"ppp","GSPI83851"

    ; default TCPIP settings for this instance
[HKEY_LOCAL_MACHINE\Comm\GSPI83851\Parms\TcpIp]
   "EnableDHCP"=dword:1
   ; This should be MULTI_SZ
   "DefaultGateway"=""
   ; Use zero for broadcast address? (or 255.255.255.255)
   "UseZeroBroadcast"=dword:0
   ; Thus should be MULTI_SZ, the IP address list
   "IpAddress"="0.0.0.0"
   ; This should be MULTI_SZ, the subnet masks for the above IP addresses
   "Subnetmask"="0.0.0.0"

;[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\GSPI8385]
;   "Order"=dword:21
;   "Dll"="GSPI8385.dll"     ; use the "streams" interface portion to load the NDIS portion
;   "Prefix"="NDL"
       ; a dd instance key for each instance that can be added
       ; "InstanceX" = "<Miniport Name>:<Miniport Instance>"
   ;"Instance0"="GSPI8385:GSPI83851"      ; first instance - must match \comm\GSPI8385X 
   ;"Instance1"="GSPI8385:GSPI83852"      ; second instance
   
[HKEY_LOCAL_MACHINE\Comm\GSPI83851\Parms]
   "PowerMode"=dword:0
   "ExtendedScan"=dword:0
   "FragThsd"=dword:2000
   "RTSThsd"=dword:2000
   "ESSID_32"=dword:1
   "Allow_Multicast"=dword:0

 