    ; registry keys for the Streams portion of the driver
[HKEY_LOCAL_MACHINE\Drivers\SDCARD\ClientDrivers\Custom\MANF-02DF-CARDID-9103-FUNC-1]
   "Dll"="SDIO8686.dll"     ; use the "streams" interface portion to load the NDIS portion
   "Prefix"="NDL"
       ; a dd instance key for each instance that can be added
       ; "InstanceX" = "<Miniport Name>:<Miniport Instance>"
   "Instance0"="SDIO8686:SDIO86861"
   
    ; registry keys for the NDIS driver
[HKEY_LOCAL_MACHINE\Comm\SDIO8686]
   "DisplayName"="Marvell SDIO8686 Wireless Card"
   "Group"="NDIS"
   "ImagePath"="SDIO8686.dll"

[HKEY_LOCAL_MACHINE\Comm\SDIO8686\Linkage]
   "Route"=multi_sz:"SDIO86861"

    ; instance 1 information
[HKEY_LOCAL_MACHINE\Comm\SDIO86861]
   "DisplayName"="Marvell SDIO8686 Wireless Card"
   "Group"="NDIS"
   "ImagePath"="SDIO8686.dll"
	
    ; instance 1 parameters
[HKEY_LOCAL_MACHINE\Comm\SDIO86861\Parms]
   "BusNumber"=dword:0
   "BusType"=dword:0

    ; TCPIP linkage to instance 1 adapter
[HKEY_LOCAL_MACHINE\Comm\Tcpip\Linkage]
    "Bind"=multi_sz:"ppp","SDIO86861"
   
    ; setup card parameters
[HKEY_LOCAL_MACHINE\Comm\SDIO86861\Parms]
   "PowerMode"=dword:0
   "ExtendedScan"=dword:1
   "FragThsd"=dword:2346
   "RTSThsd"=dword:2346
       ; following is for BT co-existence testing
   "BTMode"=dword:0
   "BTAntennaConfig"=dword:0
   "BTFrequencyConfig"=dword:0
   "BTWLANTxPriorityLo"=dword:0
   "BTWLANTxPriorityHi"=dword:0
   "BTWLANRxPriorityLo"=dword:0
   "BTWLANRxPriorityHi"=dword:0
       ; adhoc starter default channel
   "AdhocDefaultChannel"=dword:6
       ; adhoc starter WiFi test datarate modify or not 
   "AdhocWiFiDataRate"=dword:0
       ; 4Bit mode
   "SetSD4BIT"=dword:1
   "SdioIstThread"=dword:65

    ; default TCPIP settings for this instance
[HKEY_LOCAL_MACHINE\Comm\SDIO86861\Parms\TcpIp]
   "EnableDHCP"=dword:1
       ; This should be MULTI_SZ
   "DefaultGateway"=""
       ; Use zero for broadcast address? (or 255.255.255.255)
   "UseZeroBroadcast"=dword:0
       ; Thus should be MULTI_SZ, the IP address list
   "IpAddress"="0.0.0.0"
       ; This should be MULTI_SZ, the subnet masks for the above IP addresses
   "Subnetmask"="255.255.255.0"

  
