Next: Darwin Options, Previous: CRIS Options, Up: Submodel Options

#### 3.17.7 CR16 Options

These options are defined specifically for the CR16 ports.

`-mmac`
  Enable the use of multiply-accumulate instructions. Disabled by default.
`-mcr16cplus`
`-mcr16c`
  Generate code for CR16C or CR16C+ architecture. CR16C+ architecture is default.
`-msim`
  Links the library libsim.a which is in compatible with simulator. Applicable to elf compiler only.
`-mint32`
  Choose integer type as 32-bit wide.
`-mbit-ops`
  Generates sbit/cbit instructions for bit manipulations.
`-mdata-model=`model
  Choose a data model. The choices for model are ‘`near`’, ‘`far`’ or ‘`medium`’. ‘`medium`’ is default. However, ‘`far`’ is not valid when -mcr16c option is chosen as CR16C architecture does not support far data model.