Previous: MIPS Attributes, Up: GNU Object Attributes

#### 8.1.3 PowerPC Attributes

Tag_GNU_Power_ABI_FP (4)
  The floating-point ABI used by this object file. The value will be:
  - 0 for files not affected by the floating-point ABI.
  - 1 for files using double-precision hardware floating-point ABI.
  - 2 for files using the software floating-point ABI.
  - 3 for files using single-precision hardware floating-point ABI.
Tag_GNU_Power_ABI_Vector (8)
  The vector ABI used by this object file. The value will be:
  - 0 for files not affected by the vector ABI.
  - 1 for files using general purpose registers to pass vectors.
  - 2 for files using AltiVec registers to pass vectors.
  - 3 for files using SPE registers to pass vectors.