Next: Floating Point Hardware, Previous: Convenience Vars, Up: Data

### 10.12 Registers

You can refer to machine register contents, in expressions, as variables with names starting with ‘`$`’. The names of registers are different for each machine; use `info registers` to see the names used on your machine.

`info registers`
  Print the names and values of all registers except floating-point and vector registers (in the selected stack frame).

`info all-registers`
  Print the names and values of all registers, including floating-point and vector registers (in the selected stack frame).
`info registers` regname`...`
  Print the relativized value of each specified register regname. As discussed in detail below, register values are normally relative to the selected stack frame. regname may be any register name valid on the machine you are using, with or without the initial ‘`$`’.

gdb has four “standard” register names that are available (in expressions) on most machines—whenever they do not conflict with an architecture's canonical mnemonics for registers. The register names `$pc` and `$sp` are used for the program counter register and the stack pointer. `$fp` is used for a register that contains a pointer to the current stack frame, and `$ps` is used for a register that contains the processor status. For example, you could print the program counter in hex with

         p/x $pc

or print the instruction to be executed next with

         x/i $pc

or add four to the stack pointer1 with

         set $sp += 4

Whenever possible, these four standard register names are available on your machine even though the machine has different canonical mnemonics, so long as there is no conflict. The `info registers` command shows the canonical names. For example, on the SPARC, `info registers` displays the processor status register as `$psr` but you can also refer to it as `$ps`; and on x86-based machines `$ps` is an alias for the eflags register.

gdb always considers the contents of an ordinary register as an integer when the register is examined in this way. Some machines have special registers which can hold nothing but floating point; these registers are considered to have floating point values. There is no way to refer to the contents of an ordinary register as floating point value (although you can print it as a floating point value with ‘`print/f $regname`’).

Some registers have distinct “raw” and “virtual” data formats. This means that the data format in which the register contents are saved by the operating system is not the same one that your program normally sees. For example, the registers of the 68881 floating point coprocessor are always saved in “extended” (raw) format, but all C programs expect to work with “double” (virtual) format. In such cases, gdb normally works with the virtual format only (the format that makes sense for your program), but the `info registers` command prints the data in both formats.

Some machines have special registers whose contents can be interpreted in several different ways. For example, modern x86-based machines have SSE and MMX registers that can hold several values packed together in several different formats. gdb refers to such registers in `struct` notation:

         (gdb) print $xmm1
         $1 = {
           v4_float = {0, 3.43859137e-038, 1.54142831e-044, 1.821688e-044},
           v2_double = {9.92129282474342e-303, 2.7585945287983262e-313},
           v16_int8 = "\000\000\000\000\3706;\001\v\000\000\000\r\000\000",
           v8_int16 = {0, 0, 14072, 315, 11, 0, 13, 0},
           v4_int32 = {0, 20657912, 11, 13},
           v2_int64 = {88725056443645952, 55834574859},
           uint128 = 0x0000000d0000000b013b36f800000000
         }

To set values of such registers, you need to tell gdb which view of the register you wish to change, as if you were assigning value to a `struct` member:

          (gdb) set $xmm1.uint128 = 0x000000000000000000000000FFFFFFFF

Normally, register values are relative to the selected stack frame (see Selecting a Frame). This means that you get the value that the register would contain if all stack frames farther in were exited and their saved registers restored. In order to see the true contents of hardware registers, you must select the innermost frame (with ‘`frame 0`’).

However, gdb must deduce where registers are saved, from the machine code generated by your compiler. If some registers are not saved, or if gdb is unable to locate the saved registers, the selected stack frame makes no difference.

#### Footnotes

[1] This is a way of removing one word from the stack, on machines where stacks grow downward in memory (most machines, nowadays). This assumes that the innermost stack frame is selected; setting `$sp` is not allowed when other stack frames are selected. To pop entire frames off the stack, regardless of machine architecture, use `return`; see Returning from a Function.