;
; Copyright (c) Microsoft Corporation.  All rights reserved.
;
;
; Use of this source code is subject to the terms of the Microsoft end-user
; license agreement (EULA) under which you licensed this SOFTWARE PRODUCT.
; If you did not accept the terms of the EULA, you are not authorized to use
; this source code. For a copy of the EULA, please see the LICENSE.RTF on your
; install media.
;
;******************************************************************************
;*
;* System On Chip(SOC)
;*
;* Copyright (c) 2002 Software Center, Samsung Electronics, Inc.
;* All rights reserved.
;*
;* This software is the confidential and proprietary information of Samsung
;* Electronics, Inc("Confidential Information"). You Shall not disclose such
;* Confidential Information and shall use it only in accordance with the terms
;* of the license agreement you entered into Samsung.
;*
;******************************************************************************

MEMORY
;   Name     Start     Size      Type
;   -------  --------  --------  ----
    EXVECTOR 80000000  00000400  RESERVED       ; Exception vectors : used only in the bootloader (also mapped to VA 0)
    SLEEP    80000400  00000400  RESERVED       ; Sleep data - restored after wake-up
    ARGS     80000800  00001000  RESERVED       ; BSP_ARGS
    RFU0     80001800  00002800  RESERVED       ; reserved for the future use
    PTS      80004000  00004000  RESERVED       ; page table for the bootloader
    STACK    80008000  00010000  RESERVED       ; stack for the bootloader
    FLSCACHE 80020000  075E0000  RESERVED       ; Area used to cache nk.bin while programming flash
;   USB_BUF  82000000  05600000	 RESERVED       ; FLHCACHE grows while overlapping USB_BUF
    BOOTPART 87600000  00030000  RESERVED       ; BOOTPART memory (at least, 1 block + 1 sector + (sectors per block * 8))
    RFU1     87630000  000D0000  RESERVED       ; reserved for the future use
    EBOOT    87700000  00080000  RAMIMAGE       ; EBOOT code
    RFU2     87780000  00080000  RESERVED       ; reserved for the future use
    RAM	     87800000  00700000  RAM            ; RAM for bootloader
    DISPLAY  87f00000  00100000  RESERVED       ; Frame buffer

CONFIG
	COMPRESSION=OFF
	PROFILE=OFF
	KERNELFIXUPS=ON
	SRE=ON

	ROMSTART = 87700000
	ROMWIDTH = 32
	ROMSIZE  = 00080000

MODULES
;   Name            Path                                                              Memory Type
;   --------------  ----------------------------------------------                    -----------
    nk.exe          $(_TARGETPLATROOT)\target\$(_TGTCPU)\$(WINCEDEBUG)\eboot.exe      EBOOT

